MeshMini (MeshLink BBS)

User Cheat Sheet — v0.9.2

# Commands

|  |  |  |
| --- | --- | --- |
| Command | What it does | Example |
| ? / menu / m | Show the notice (if any) and a compact one-line menu. | m |
| ?? / help / h | Show detailed help. | ?? |
| r | List recent posts (paged automatically). | r |
| r <id> | Read a specific post and its replies. | r 12 |
| p <text> | Post a new message. | p Kia ora Hawke’s Bay! |
| reply <id> <text> | Reply to a post by ID. | reply 12 Thanks! |
| info | Show the current notice, with Set/Expires times. | info |
| status | Show this node’s long name / short name / uptime. | status |
| whoami | Show your node ID and names. | whoami |
| nodes | List visible nodes (shortName, nodeId, longName). | nodes |
| whois <short> | Look up a node by short name (fuzzy matching). | whois GN4B |
| dm <short> <text> | Queue a direct message; delivered when the node is seen. | dm GN4B Meet at the top gate |

# Notes

• The one-line menu auto-shrinks to fit your device’s text limit (default MAX\_TEXT=140).

• Long outputs (like node lists or threads) are automatically paginated.

• Unknown/telemetry noise is ignored; human-like unknowns get a friendly hint (if enabled by admin).

• Rate limiting: default 2s between messages per sender (MMB\_RATE).